1.

netsh interface show interface

2.

netsh interface ip set address name= "Loopback Pseudo-Interface 1" static 192.168.123.15 255.255.255.0 192.168.1.1

netsh interface ip set dnsservers name="Loopback Pseudo-Interface 1" static 8.8.8.8 primary validate=no

netsh interface ip add dnsservers name= "Loopback Pseudo-Interface 1" address=8.8.4.4 index=2 validate=no

3. ping youtube.com

4. tracert [www.google.com](http://www.google.com)

//after doing changes to loopback pseudo interface again change it to original one configuration as it causes problem with localhost ports.